How to mount/dismount EX1 chassis panels

Created by: David Rodriguez ([davidrm@dc.tohoku.ac.jp](mailto:davidrm@dc.tohoku.ac.jp))

Last update: Jan. 9, 2020

Updated by: David Rodriguez

# Mounting Operation

1. First mount the side panels.
   1. Attached the rocker sensor support structure to the side panel.
   2. Pass all the cables through the support structure first and then through the center hole in the panel.
   3. Mount the panel to the chassis.
   4. Connect cables to the Rocker Interface Unit (RIU)
2. Next, mount the top panel. You will need free access through the front and back to tighten the nuts of the top panel.
3. Attach the back panel.
4. Last mount the front panel to the chassis.

*NOTE: For the dismounting operation simply follow the previous steps in the reverse order.*